Author: Dlee

Technical Data Sheet
Materials Specifications For:
Plateform Mount Series: EP3002

Applications
Oxygen concentrators
Gensets
Engine mounts
Cab mounts
Medical equipment
Compressors
Electronic equipment

Attributes
All attitude
Low cost
Compact, low profile design
Available in a square or diamond shaped flange
Easy to install
Low natural frequency

Load Range
EP3001 = 8 load ratings from 4 to 20 lbs.
EP3002 = 16 load ratings from 3 to 26 lbs.
EP3003 = 10 load ratings from 12 to 60 lbs.
EP3004 = 12 load ratings from 20 to 90 lbs.
EP3106 = 10 load ratings from 1 to 6 lbs.
EP3156 = 8 load ratings from 6 to 16 lbs.

Specifications
Natural frequency—8-20 Hertz
Transmissibility at resonance—10:1
Resilient element—Neoprene
Standard materials—Cold-rolled steel
Weight—varies with model

Elastomeric Data
Neoprene has an operating temperature range of -40°F to +200°F (-40°C to +93°C) and is resistant to oil, most solvents and ozone
Other elastomeric formulations are available in BUNA-N, Silicone, Butyl and Polybutadiene for improved damping, low and high temperature resistance

Page 1 of 2

Technical Data Sheet
Materials Specifications For:
Plateform Mount Series: EP3002

Diamond Flange

PART / NUMBER	MAXIMUM / STATIC / (lbs.)	AXIAL SPRING RATE / (lbs./in.)
EP3002-01	3	33
EP3002-02	6	63
EP3002-03	9	100
EP3002-04	12	130
EP3002-05	14	163
EP3002-06	17	192
EP3002-07	20	220
EP3002-08	26	290

Square Flange

PART / NUMBER	MAXIMUM / STATIC / (lbs.)	AXIAL SPRING RATE / (lbs./in.)
EP3002-51	3	33
EP3002-52	6	63
EP3002-53	9	100
EP3002-54	12	130
EP3002-55	14	163
EP3002-56	17	192
EP3002-57	20	220
EP3002-58	26	290

Page 2 of 2

Specifications subject to change without notice. Check with factory for latest revisions. The Federal Trade Commission considers no existing test methods or standards regarding flammability as accurate indictors of the performance of cellular plastic materials under actual fire conditions. Results of existing test methods, such as UL-94, MVSS-302, SAE J-369, and FAR 25.853 are intended only as measurements of the performance of such materials under specific controlled test conditions. Any flammability ratings shown are not intended to reflect hazards presented by these materials under actual fire conditions. The information contained herein is based on laboratory test data developed for PTI and is believed to be reliable, but its accuracy or completeness is not guaranteed. The buyer must test any product to determine the suitability for h is specific application before use. PTI DISCLAIMS ANY RESPONSIBILITY FOR: 1) WARRANTIES OF FITNESS AND PURPOSE, 2) VERBAL RECOMMENDATIONS, 3) CONSEQUENTIAL DAMAGES FROM USE AND 4) VIOLATION OF ANY PATENTS OF TRADEMARKS HELD BY OTHERS.
420 Corporate Blvd., Newark, DE 19702 - Phone: 302/738-9001- Fax: 302/738-9085
www.polytechinc.com

Specifications subject to change without notice. Check with factory for latest revisions. The Federal Trade Commission considers no existing test methods or standards regarding flammability as accurate indictors of the performance of cellular plastic materials under actual fire conditions. Results of existing test methods, such as UL-94, MVSS-302, SAE J-369, and FAR 25.853 are intended only as measurements of the performance of such materials under specific controlled test conditions. Any flammability ratings shown are not intended to reflect hazards presented by these materials under actual fire conditions. The information contained herein is based on laboratory test data developed for PTI and is believed to be reliable, but its accuracy or completeness is not guaranteed. The buyer must test any product to determine the suitability for h is specific application before use. PTI DISCLAIMS ANY RESPONSIBILITY FOR: 1) WARRANTIES OF FITNESS AND PURPOSE, 2) VERBAL RECOMMENDATIONS, 3) CONSEQUENTIAL DAMAGES FROM USE AND 4) VIOLATION OF ANY PATENTS OF TRADEMARKS HELD BY OTHERS.
420 Corporate Blvd., Newark, DE 19702 - Phone: 302/738-9001- Fax: 302/738-9085
www.polytechinc.com